Hej

Här kommer dokumentet som beskriver hur ni ska få ICQ att fungera.

Om ni följer detta dokument på dator nummer två så måste ni byta portarna till 25010-25015

När detta dokument är klart ska ni öppna Internet explorer och logga in med användarnamn: admin och lösenord: 1234

Sedan klickar ni på advanced och ports.Där skriver ni in de portar som ni redan har matat in i ICQn för dator ett och sedan lika på nästa

rad för dator två och sedan IP adressen till respektive dator. Exempel: Start port: 24500 End port: 24505 server IP adress: 192.168.0.2

  

Best Regards 
Jonas Asplund

Netgear Support Sweden 
www.netgear.com 
Technical Support (Sweden) 0200 - 298 298 

THE ICQ-FIX !! :

In this example I´m going to use ports 24500-24505..
.. but you can choose whatever ports you want..
You find these settings under: Main > Preferences > Connections


1. Use the ICQ ports above above, or change them.

2. Change to "Using Proxy" and select "Socks 4" (see below) 
(You must do this! ..I know that you are not using proxy for
connecting to the internet..but this is the thing that"removes" the bug !
..we will change back later...) 
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3. Apply and restart ICQ
(ONLY change to SOCKS4 under "User")

4. Now you will se a listening port in that area you specified
(use netstat if you want to examin that. )

5. and now you should change back to "Specified Ports" in ICQ
and it will stay there for you (see below)...
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6. Done !..right now ICQ setup is function correct..
 Then all that is needed is to open the ports in your
gateway/router 

